# Dymo-printed labels

## On regulator knob

SP: 15-20 psig

## Next to valve label, below tray slot/handle

🡨 WAIT FOR **ZERO** PRESSURE  
 BEFORE TURNING OFF

## On mass flow controller

RANGE: 0.005 to 1.000 SLPM

Valve

Always open or close **FIRST**